Highlights

Topological interlocking does not rely on the material's tendency to deform

Topological interlocking can satisfy extrusion continuity constraints

Which lattice is strongest depends on the space available for interlocking

The tensile strength of any interlock cannot exceed a theoretical upper bound

Tensile properties of our lattice can are well approximated by analytical models